Issued to:		Matchmaster Dyeing & Finishing, Inc, Dba Antex Knitting Mills	
		3700 S. Broadway
Los Angeles, CA  90007
USA	
			
This is to certify that
representative samples of		Component – Textile Fabrics for Protection of Industrial Personnel Against Flash Fire	
		See Page 2	
			
		Have been investigated by UL in accordance with the Standard(s) indicated on this Certificate.	
			
Standard(s) for Safety:		NFPA 2112, Standard on Flame-Resistant Garments for Protection of Industrial Personnel Against Flash Fire, 2012 Edition	
Additional Information:		See the UL Online Certifications Directory at www.ul.com/database for additional information	

Only those products bearing the UL Recognized Component Mark should be considered as being covered by UL's Recognition and Follow-Up Service.
The UL Recognized Component Mark generally consists of the manufacturer’s identification and catalog number, model number or other product designation as specified under “Marking” for the particular Recognition as published in the appropriate UL Directory.  As a supplementary means of identifying products that have been produced under UL’s Component Recognition Program, UL’s Recognized Component Mark: , may be used in conjunction with the required Recognized Marks.  The Recognized Component Mark is required when specified in the UL Directory preceding the recognitions or under “Markings” for the individual recognitions.
Recognized components are incomplete in certain constructional features or restricted in performance capabilities and are intended for use as components of complete equipment submitted for investigation rather than for direct separate installation in the field.   The final acceptance of the component is dependent upon its installation and use in complete equipment submitted to UL LLC.

Look for the UL Recognized Component Mark on the product.

The following materials have been found to be in compliance.

Outer Shell Fabrics:  1580FR, 1852FM, 8581FR, 3108FW, 865HFR, 1582FW, 545CFM, 322XFR, 1950FM, 5601FP, 8812FR

Other Textile Materials (Collar, Cuff): 168LFR, 2176FR